Stylianou et al., 2017

* Heat exchange rate larger when lithology with high thermal conductivity and presence of groundwater.
* Development of a tool to measure and analyse the thermal properties of lithologies encountered in an area used to predict heat injection rate of a GHE (depending on its characteristics, GW flow and ground properties)
* Tool can be used to size GHE and calculate heat injection rate in any areas